|  |
| --- |
| **Equipment Inspection Form** |

|  |  |
| --- | --- |
| Skipper (full name) | Click here to edit |
| Crew (full name) | Click here to edit |
| Sail Number | Click here to edit |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  | Competitor Use |  | Official Use - Check |
|  |  |  |  |  |  |
| **Boat** | Weight (min 141 kg) |  |  |  | (kg) |
|  | Corrector Weight |  |  |  | (kg) |
| **Beam** | Flex (5 – 9 mm) |  |  |  |  (mm) |
|  |  |  |  |  |  |
| **Hull** | Hull Number (HIN) |  | Click here to edit |  |  |
|  |  |  |  |  |  |
| **Foils** | STB Dagger Serial |  | Click here to edit |  |  |
|  | PRT Dagger Serial |  | Click here to edit |  |  |
|  | STB Rudder Serial |  | Click here to edit |  |  |
|  | PRT Rudder Serial |  | Click here to edit |  |  |
|  |  |  |  |  |  |
| **Sails** | Mainsail Serial |  | Click here to edit |  |  |
|  | Jib Serial |  | Click here to edit |  |  |
|  | Spinnaker Serial |  | Click here to edit |  |  |
|  |  |  |  |  |  |
| **Parts** | Following parts have their certification labels:  |  | MastBoomFront Beam Rear Beam BowspritBridles Spreaders Compression strut |  | OK / NOKOK / NOKOK / NOKOK / NOKOK / NOKOK / NOKOK / NOKOK / NOK |
|  |  |  |

**SKIPPER’S DECLARATION**

* 1. I understand that these items may not be substituted or repaired at any time during the event without prior written consent of the Event Inspector as permitted by Equipment Regulation 3.
	2. It is my sole responsibility (RR 78) to ensure that the equipment I use for this event shall comply with the class rules at all times and that the equipment may be checked for class rule compliance at any time during the event.

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date Signature

**Instructions on Equipment Limitation Stickers**

Inspection Team must ensure that equipment is;

* DRY & CLEAN

**BEFORE** apply the stickers to any item of equipment !!

Please ensure that stickers are placed according to the instructions below. Keep in mind that all stickers should be clearly visible to the Equipment Inspection Team.

**HULLS –Sticker serial number 01/02**

Place on each transom.

**MAST –Sticker serial number 03**

Place on the port side of the mast between the gooseneck and the deck.

Ensure sticker is clear of any rigging or attachments.

**DAGGERBOARDS-Sticker serial number 04/05**

Place on top of board whereby sticker may be seen without the need to remove from hull.

**RUDDER BLADES- Sticker serial number 06/07**

Place on top of blade whereby sticker may be seen without the need to remove from housing.

**BOOM – Sticker serial number 08 (optional)**

Place on the port aft end of the boom such that sticker is stuck along the length of the pole. Ensure sticker is clear of any rigging or attachments.

**NOTE – This form shall be returned to the World Sailing appointed, Equipment Inspector.**